Tayorcraft BC12-D 
X-Plane 9.7
Author: Barry Roberts 
Email: xplanebaz@aapt.net.au 
Version: 1.1
Date: 5 November 2013


Installation:
Copy the entire aircraft folder into the aircraft folder in X-Plane 

Copyright: 2013
Don't publish any modified or altered version without my consent.

Crew: one
Capacity: one passenger
Empty weight: 860 lb (390 kg)
Gross weight: 1,500 lb (680 kg)
Fuel capacity: 18 U.S. gallons (68 L; 15 imp gal)
Powerplant: 1 × Continental C-85 four-cylinder horizontally opposed aircraft engine, 85 hp (63 kW)

Performance
Maximum speed: 120 mph (193 km/h; 104 kn)
Cruise speed: 110 mph (96 kn; 177 km/h)
Stall speed: 38 mph (33 kn; 61 km/h)
Range: 300 mi (261 nmi; 483 km)
Service ceiling: 17,000 ft (5,182 m)
Rate of climb: 700 ft/min (3.6 m/s)


Comments and feedback welcome
Barry
