BEFORE ENGINE STARTING
Parking Brake - SET
Landing Gear Control - CHECK DOWN
Power Levers - IDLE
Propeller Controls - FULL FORWARD
Condition Levers - FUEL CUTOFF
Fuel Quantity - CHECK
Anti-ice - ON if OAT < 4C (39F)
Beacon - ON

ENGINE STARTING
Battery Switch  - ON
Beacon  - ON
Propeller Area  - CLEAR
Fuel Flow  - ON
Left Ignition and Engine Start Switch - ON
Left Condition Lever  - LOW IDLE
Left ITT and N1 Turbine RPM  - MONITOR
L FUEL PRESS LO Annunciator  - EXTINGUISHED
L OIL PRESS LO Annunciator  - EXTINGUISHED
Left Oil Pressure  - CHECK
Left Condition Lever  - HIGH IDLE
Left Generator  - ON
Left Ignition and Engine Start Switch - ON
Right Condition Lever  - LOW IDLE
Right ITT and N1 Turbine RPM  - MONITOR
R FUEL PRESS LO Annunciator  - EXTINGUISHED
R OIL PRESS LO Annunciator  - EXTINGUISHED
Right Oil Pressure  - CHECK
Right Condition Lever  - HIGH IDLE
Right Condition Lever  - REDUCE TO LOW IDLE
Right Generator  - ON
Avionics Master Switch  - ON

BEFORE TAKEOFF
Avionics - CHECK
Autopilot - ADJUST HEADING AND FL
Electronic Pitch Trim Control - NEUTRAL
Trim Tab - SET
Primary Governors - EXERCISE AT 1800 RPM (80%)
Autofeather - ARM
Manual Propeller Feathering - CHECK
Anti-ice - AS REQUIRED
Fuel Quantity, Flight, and Engine Instruments - CHECK

BEFORE TAKEOFF
Annunciator Lights  - EXTINGUISHED OR CONSIDERED
Transponder  - ON ALT
Lights  - AS REQUIRED
Anti-ice  - AS REQUIRED
Takeoff speeds (V1, VR, and V2)  - CONFIRM
Ê
TAKEOFF
Brakes - HOLD
Power Levers - 100% N1 TURBINE RPM
Brakes - RELEASE
VR - ROTATE TO APPROX. 10 DEGREES PITCH UP
Landing Gear - UP
Airspeed - MAINTAIN V2 UNTIL CLEAR OF OBSTACLES
Flaps - UP (BLUE LINE, 125 KIAS MINIMUM)


CLIMB - 160 KIAS recommendedÊ
Climb Power  - 91% N1 TURBINE RPM
Propellers - 2200 RPM (95%)
Propeller Synchrophaser  - ON
Engine Instruments  - MONITOR
Lights  - AS REQUIRED

CRUISEÊ
Cruise Power - AS DESIRED
Engine Instruments - MONITOR
Autofeather - OFF

DESCENT
Altimeter - SET
Autofeather - ARM
Fuel Balance - CHECK
Power - AS REQUIRED

BEFORE LANDING 
Autofeather - VERIFY ARMED
VREF - CONFIRM
Altimeter - SET
Flaps - AS REQUIRED
Landing Gear - DOWN 
Lights - AS REQUIRED
Anti-ice - AS REQUIRED

LANDING
Flaps - DOWN
Airspeed - VREF
Condition Levers - HIGH IDLE
Propeller Levers - FULL FORWARD
Power Levers - IDLE

AFTER TOUCHDOWN
Power Levers - REVERSE
Brakes - AS REQUIRED

AFTER LANDING
Engine Auto-Ignition  - OFF
Anti-ice  - OFF
Lights  - AS REQUIRED
Transponder  - STANDBY
Trim Tabs  - SET
Flaps  - UP

SHUTDOWN AND SECURING
Parking Brake  - SET
Avionics Master  - OFF
Autofeather  - OFF
Lights  - OFF
ITT  - STABILIZED AT MINIMUM TEMPERATURE FOR 1 MINUTE
Condition Levers  - FUEL CUTOFF
Propellers  - FEATHER
Battery and Generator Switches  - OFF (below 15% N1)
