Cessna T303 Crusader
X-Plane 9.7
Author: Barry Roberts 
Email: xplanebaz@aapt.net.au 
Version: 2.2
Date: 13 October 2013


Installation:
Copy the entire aircraft folder into the aircraft folder in X-Plane 

Copyright: 2013
Don't publish any modified or altered version without my consent.

Engines
Teledyne Continental Engines:	Left - TSIO-520 AE
	Right - LTSIO-520 AE
 
Turbocharged, direct-drive, air-cooled, horizontally opposed, fuel injected, six cylinder, 520CC, 250 Brake Horse Power at 2400 Rpm at sea level.
 
Propellers
McCauley, Max. diameter 74 inch, Min. diameter 72,5 inch.
Constant speed, full-feathering, non-reversible, hydraulically actuated.
Low pitch: 18,7¡-19,6¡
Feathered: 80¡-81,3¡
 
Fuel
Fuel types allowed:	100 LL
	100 Grade aviation fuel Green (100/130)
 
Fuel Capacity
155 US Gallons, (77,5 US Gallons Left, 77,5 US Gallons Right)
Total usable fuel: 153 US Gallons

Dimensions
Width : 12 meters
Length : 9 meters, 30 centimeters
Height : 4 meters, 10 centimeters
Ground clearance : 30 centimeters
 
Maximum allowable masses:
Maximum Ramp Mass : 5175 Lbs
Maximum Take Off Mass : 5150 Lbs
Maximum Landing Mass : 5150 Lbs (Heavy Duty)
Maximum Zero Fuel Mass : 4850 Lbs
 
Baggage Limitations
Aft baggage limit: 200 Lbs
Nose locker limit : 150 Lbs
Wing locker limit : 120 Lbs (max. 60 Lbs under locker doors)
Aircraft Limitations
 
Speeds
Vne : 210 Kias 
Vle : 210 Kias
Vno : 175 Kias 
Vlo : 175 Kias - extension
Va:	133 Kias at 4150 Lbs 
	148 Kias at 5150 Lbs
	150 Kias - retraction
	141 Kias at 4650 Lbs 
Vmca: 65 Kias
Vso : 58 Kias
Vfe: 	175 Kias with 10¡ Flaps 
	150 Kias with 20¡ Flaps 
	125 Kias with 30¡ Flaps
Vs : 66 Kias (max. fwd C.of G.)
Vy : 103 Kias
Vy se : 97 Kias
Vx se : 93 Kias


Comments and feedback welcome
Barry
