

CARB HEAT

FUEL SHUT OFF

THROTTLE PRIMER

CABIN HEAT MIXTURE

Battery

START

BOTH

R

L

OFF