###----------------------------------------------------###
### Checklist for CessnaT303v10.51   XP10              ###
### Vers.3.0                                           ###
### To be used with Xchecklist Plugin                  ###
### Checklist created by xplanebaz@aapt.net.au         ###
###----------------------------------------------------###

sw_checklist:Aircraft Acceptance - CessnaT303
sw_item:Maintenance Status|Check

sw_checklist:01 START CHECKS:START CHECKS
sw_item:Maintenance Status|CHECK
sw_item:Walk around|CHECK
sw_item:Hobbs Meter|CHECK
sw_item:Adjust seat, fasten belts|CHECK:sim/cockpit2/switches/fasten_seat_belts:1
sw_item:Lock doors |CLOSED:sim/cockpit2/switches/door_open[4]:1
sw_item:Gear switch down|DOWN:sim/cockpit2/controls/gear_handle_down:1
sw_item:Avionics|OFF:sim/cockpit2/switches/avionics_power_on:0
sw_item:Generators |ON:(sim/cockpit2/electrical/generator_on[0]:1)&&(sim/cockpit2/electrical/generator_on[1]:1)
sw_item:Battery|ON:sim/cockpit2/electrical/battery_on:1
sw_item:Circuit breakers|IN
sw_item:Fuel quantity|CHECK
sw_item:Left fuel selector|ON:sim/cockpit2/fuel/fuel_tank_selector:4
sw_item:Right fuel selector|ON:sim/cockpit2/fuel/fuel_tank_selector:4
sw_item:Elevator trim|TAKE OFF:sim/flightmodel/controls/elv_trim:0
sw_item:Rudder trim|NEUTRAL:sim/cockpit2/controls/rudder_trim:0
sw_item:Aileron trim|NEUTRAL:sim/cockpit2/controls/aileron_trim:0
sw_item:Altimeter & clock|CHECK
sw_item:Release parking brake, check brakes|CHECK:sim/flightmodel/controls/parkbrake:0
sw_item:Parking brake|CHECK:sim/flightmodel/controls/parkbrake:1
sw_item:Beacon|ON:sim/cockpit2/switches/beacon_on:1
sw_item:Night flight lights & flashlight|CHECK
sw_continue



sw_checklist:02 START - LEFT:START - LEFT
sw_item:Mixture|FULL RICH:sim/flightmodel/engine/ENGN_mixt[0]:1
sw_item:Propeller|FINE:(sim/cockpit2/engine/actuators/prop_rotation_speed_rad_sec[0]:>200)
sw_item:Open throttle 1/2 inch |SET:sim/cockpit2/engine/actuators/throttle_ratio[0]:>0.1
sw_item:Mags|ON:sim/cockpit2/engine/actuators/ignition_on[0]:3
sw_item:Clear prop |CHECK
sw_item:Boost pumps|ON:sim/cockpit2/engine/actuators/fuel_pump_on[0]:1
sw_item:Starter button|ENGAGED
sw_item:Oil pressure (30 sec hot, 60 sec cold) |CHECK
sw_continue



sw_checklist:03 START - RIGHT:START - RIGHT
sw_item:Mixture|FULL RICH:sim/flightmodel/engine/ENGN_mixt[1]:1
sw_item:Propeller|FINE:(sim/cockpit2/engine/actuators/prop_rotation_speed_rad_sec[1]:>200)
sw_item:Open throttle 1/2 inch |SET:sim/cockpit2/engine/actuators/throttle_ratio[1]:>0.1
sw_item:Mags|ON:sim/cockpit2/engine/actuators/ignition_on[1]:3
sw_item:Clear prop |CHECK
sw_item:Boost pumps|ON:sim/cockpit2/engine/actuators/fuel_pump_on[1]:1
sw_item:Starter button|ENGAGED
sw_item:Oil pressure (30 sec hot, 60 sec cold) |CHECK
sw_item:Avionics |ON:sim/cockpit2/switches/avionics_power_on:1
sw_item:Transponder|STANDBY:sim/cockpit/radios/transponder_mode:1
sw_item:Taxi light|ON:sim/cockpit2/switches/taxi_light_on:1
sw_continue



sw_checklist:04 WARM-UP & CHECK:WARM-UP & CHECK
sw_item:Both engine to 800-1000 RPM|SET:(sim/cockpit2/engine/indicators/engine_speed_rpm[0]:>800)&&(sim/cockpit2/engine/indicators/engine_speed_rpm[1]:>800)
sw_item:Boost pumps|OFF to check engine pumps, then ON:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:1)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:1)
sw_item:Left engine RPM|1700:sim/cockpit2/engine/indicators/engine_speed_rpm[0]:>1600
sw_item:Engine instruments|CHECK
sw_item:Generators |OFF, then ON noting voltage
sw_item:Check vacuum pumps|CHECK
sw_item:Check magnetos|MAX 200 RPM DROP:sim/cockpit2/engine/actuators/ignition_on[0]:2
sw_item:Cycle prop|RPM drops to 1000
sw_item:Check oil pressure |30-60 PSI
sw_item:Left engine to 800-1000 RPM|SET:(sim/cockpit2/engine/indicators/engine_speed_rpm[0]:<1200)
sw_item:Right engine RPM|1700:sim/cockpit2/engine/indicators/engine_speed_rpm[1]:>1600
sw_item:Check engine instruments|CHECK
sw_item:Check generators |OFF, then ON noting voltage
sw_item:Check vacuum pumps|CHECK
sw_item:Check annunciator panel|CHECK:sim/cockpit/warnings/annunciator_test_pressed
sw_item:Check magnetosMAX 200 RPM DROP:sim/cockpit2/engine/actuators/ignition_on[1]:2
sw_item:Cycle prop|RPM drops to 1000
sw_item:Left engine to 800-1000 RPM|SET:(sim/cockpit2/engine/indicators/engine_speed_rpm[1]:<1200)
sw_continue

sw_checklist:05 PREFLIGHT CHECK:PREFLIGHT CHECK
sw_item:Parking brake|SET:sim/flightmodel/controls/parkbrake:1
sw_item:Flight controls|FREE & CORRECT
sw_item:Elevator trim|TAKE OFF:sim/flightmodel/controls/elv_trim:0
sw_item:Rudder trim|NEUTRAL:sim/cockpit2/controls/rudder_trim:0
sw_item:Aileron trim|NEUTRAL (vis check):sim/cockpit2/controls/aileron_trim:0
sw_item:Propeller|FINE:(sim/cockpit2/engine/actuators/prop_rotation_speed_rad_sec[0]:>200)
sw_item:Boost pumps|ON:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:1)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:1)
sw_item:Cabin door & window|CLOSED & LOCKED
sw_item:Transponder|MODE C:sim/cockpit/radios/transponder_mode:2
sw_item:Landing light and Strobes|ON:(sim/cockpit2/switches/landing_lights_on[0]:1)&&(sim/cockpit2/switches/landing_lights_on[1]:1)&&(sim/cockpit2/switches/strobe_lights_on:1)
sw_item:Cowl flaps|OPEN:(sim/cockpit2/engine/actuators/cowl_flap_ratio[0]:>0.7)&&(sim/cockpit2/engine/actuators/cowl_flap_ratio[1]:>0.7)
sw_item:Flaps |0-15:(sim/cockpit2/controls/flap_ratio:>0.05)&&(sim/cockpit2/controls/flap_ratio:<0.50)
sw_continue



sw_checklist:06 TAKE-OFF:TAKE-OFF
sw_itemvoid:Normal Take-Off |Vmc = 65 Kias
sw_item:Throttles to full power|POWER SET:(sim/flightmodel/engine/ENGN_thro[0]:>.95)&&(sim/flightmodel/engine/ENGN_thro[1]:>.95)
sw_item:Rotate|97 Kias:sim/cockpit2/gauges/indicators/airspeed_kts_pilot:>95
sw_item:Apply brakes |CHECK:sim/cockpit2/controls/left_brake_ratio:1
sw_item:Gear|UP:sim/flightmodel2/gear/deploy_ratio[0]:0
sw_item:Taxi light|OFF:sim/cockpit2/switches/taxi_light_on:0
sw_item:Accelerate |103 Kias (Vy):sim/cockpit2/gauges/indicators/airspeed_kts_pilot:>100
sw_item:Flaps|RETRACT:sim/cockpit2/controls/flap_ratio:<0.10
sw_item:Boost pumps|OFF:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:0)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:0)
sw_continue



sw_checklist:07 CLIMB:CLIMB
sw_item:Normal climb|110Kias, MP 24, RPM 2450
sw_item:MP|CHECK ON CLIMB
sw_item:Cowl flaps|CLOSED 500ft BEFORE TOC:(sim/cockpit2/engine/actuators/cowl_flap_ratio[0]:0)&&(sim/cockpit2/engine/actuators/cowl_flap_ratio[1]:0)
sw_item:Seat belts |AS REQD:sim/cockpit2/switches/fasten_seat_belts:0
sw_continue



sw_checklist:08 CRUISE:CRUISE
sw_item:Normal cruise|MP 23, RPM 2300
sw_item:Trim |CHECK
sw_item:Lean each engine separately |EGT 100 deg rich of peak
sw_item:Propellers |SYNCHRONIZED:sim/cockpit2/switches/prop_sync_on:1
sw_item:Radios|TUNED AND SET
sw_item:Autopilot|CHECK AND SET
sw_item:Fuel quantity |CHECK

sw_checklist:09 LET DOWN:LET DOWN
sw_item:Maintain cruising speed @ cruise rpm|CHECK
sw_item:ATIS/Airport info|CHECK
sw_item:Altimeter|CHECK
sw_item:Mixture controls|ENRICH ON DESCENT:(sim/flightmodel/engine/ENGN_mixt[0]:1)&& (sim/flightmodel/engine/ENGN_mixt[1]:1)
sw_continue

sw_checklist:10 BEFORE LANDING:BEFORE LANDING
sw_item:Brakes|CHECK:sim/cockpit2/controls/left_brake_ratio:1
sw_item:Gear|DOWN:sim/cockpit/switches/gear_handle_status:1
sw_item:Propellers Synchronizer|OFF:sim/cockpit2/switches/prop_sync_on:0
sw_item:Mixture|FULL RICH:(sim/flightmodel/engine/ENGN_mixt[0]:1)&& (sim/flightmodel/engine/ENGN_mixt[1]:1)
sw_item:Boost pumps|ON:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:1)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:1)
sw_item:Flaps|10-20:sim/cockpit2/controls/flap_ratio:<0.25
sw_item:Seat belts|CHECK:sim/cockpit2/switches/fasten_seat_belts:1
sw_continue

sw_checklist:11 PUFF CHECK:PUFF CHECK
sw_item:Propeller|FINE:(sim/cockpit2/engine/actuators/prop_rotation_speed_rad_sec[0]:>200)&&(sim/cockpit2/engine/actuators/prop_rotation_speed_rad_sec[1]:>200)
sw_item:Gear|CHECK:(sim/cockpit2/controls/gear_handle_down:1)&&(sim/flightmodel2/gear/deploy_ratio[0]:1)&&(sim/flightmodel2/gear/deploy_ratio[1]:1)&&(sim/flightmodel2/gear/deploy_ratio[2]:1)
sw_item:Taxi light|ON:sim/cockpit2/switches/taxi_light_on:1
sw_item:Flaps|20-30:sim/cockpit2/controls/flap_ratio:<0.50
sw_item:Cowl flaps|OPEN:(sim/cockpit2/engine/actuators/cowl_flap_ratio[0]:>0.8)&&(sim/cockpit2/engine/actuators/cowl_flap_ratio[1]:>0.8)
sw_item:Trim tab|AS REQÕD
sw_item:Landing lights|ON:(sim/cockpit/electrical/landing_lights_on[0]:1)&&(sim/cockpit/electrical/landing_lights_on[1]:1)

sw_checklist:12 TAXI TO RAMP:TAXI TO RAMP
sw_item:Retract flaps|0:sim/cockpit2/controls/flap_ratio:0
sw_item:Boost pumps|OFF:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:0)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:0)
sw_item:Strobe lights|OFF:sim/cockpit/electrical/strobe_lights_on:0
sw_item:De-ice|OFF
sw_item:Cowl flaps|CLOSED:(sim/cockpit2/engine/actuators/cowl_flap_ratio[0]:<0.4)&&(sim/cockpit2/engine/actuators/cowl_flap_ratio[1]:<0.4)
sw_item:Elevator trim set|TAKEOFF:sim/flightmodel/controls/elv_trim:0.0
sw_item:Radio|AS REQÕD
sw_item:Landing lights|OFF:(sim/cockpit/electrical/landing_lights_on[0]:0)&&(sim/cockpit/electrical/landing_lights_on[1]:0)
sw_item:Transponder|1200 Stby:sim/cockpit/radios/transponder_mode:1
sw_continue



sw_checklist:13 SHUTDOWN:SHUTDOWN
sw_item:Parking brake|SET:sim/flightmodel/controls/parkbrake:1
sw_item:Throttle|IDLE:(sim/flightmodel/engine/ENGN_thro[0]:<0.4)&&(sim/flightmodel/engine/ENGN_thro[1]:<0.4)
sw_item:Boost pumps|OFF:(sim/cockpit2/engine/actuators/fuel_pump_on[0]:0)&&(sim/cockpit2/engine/actuators/fuel_pump_on[1]:0)
sw_item:Cabin heater|OFF
sw_item:Beacon light|OFF:sim/cockpit/electrical/beacon_lights_on:0
sw_item:Taxi lights|OFF:sim/cockpit/electrical/taxi_light_on:0
sw_item:Pitot heat|OFF:sim/cockpit/switches/pitot_heat_on:0
sw_item:Avionics|OFF:sim/cockpit/electrical/avionics_on:0
sw_item:Generator|OFF:(sim/cockpit2/electrical/generator_on[0]:0)&&(sim/cockpit2/electrical/generator_on[1]:0)
sw_item:Mixture|CUTOFF:(sim/flightmodel/engine/ENGN_mixt[0]:<0.5)&& (sim/flightmodel/engine/ENGN_mixt[1]:<0.5)
sw_item:Mags|OFF:(sim/cockpit2/engine/actuators/ignition_on[0]:0)&&(sim/cockpit2/engine/actuators/ignition_on[0]:0)
sw_item:Seatbelts |OFF:sim/cockpit2/switches/fasten_seat_belts:0
sw_item:Battery|OFF:sim/cockpit/electrical/battery_on:0

sw_checklist:14 GO-AROUND:GO-AROUND
sw_item:Full throttle, RPM 2600 |SET:(sim/flightmodel/engine/ENGN_thro[0]:>0.8)&&(sim/flightmodel/engine/ENGN_thro[1]:>0.8)
sw_item:Landing gear|UP:(sim/cockpit2/controls/gear_handle_down:1)
sw_item:Flaps|RETRACT TO 15:sim/cockpit2/controls/flap_ratio:0.4
sw_item:Trim |CLIMB
sw_item:Flaps|RETRACT WHEN SAFE: sim/cockpit2/controls/flap_ratio:0

sw_checklist:Important Speeds:Important Speeds
sw_itemvoid:Vne 210 Kias
sw_itemvoid:Vno 175 Kias
sw_itemvoid:Va:	133 Kias at 4150 Lbs 
sw_itemvoid:	148 Kias at 5150 Lbs
sw_itemvoid:	150 Kias - retraction
sw_itemvoid:	141 Kias at 4650 Lbs 
sw_itemvoid:Vfe: 	175 Kias with 10ø Flaps 
sw_itemvoid:	150 Kias with 20ø Flaps 
sw_itemvoid:	125 Kias with 30ø Flaps
sw_itemvoid:Vle 210
sw_itemvoid:Vmca: 65 Kias
sw_itemvoid:Vy : 103 Kias
sw_itemvoid:Vyse : 97 Kias
sw_itemvoid:Vxse : 93 Kias
sw_itemvoid:Vs : 66 Kias (max. fwd C.of G.)
sw_itemvoid:Vso : 62 Kias
sw_item:Finished


