Bellanca Super Viking 300A
For X-Plane 10.30
Author: Barry Roberts
Email: xplanebaz@aapt.net.au
Version: 3.1
Date: 22-Nov-2014

Installation:
Copy the entire aircraft folder into the aircraft folder in X-Plane 

Copyright: 2014
Don't publish any modified or altered version without my consent.

Aircraft Specs:
Wing span: 34 ft 2 in (10.41 m)
Length overall: 26 ft 4 in (8.02 m)
Height overall: 7 ft 4 in (2.24 m)
Tailplane span: 12 ft 2 in (3.71 m)
Wheel track: 9 ft 0 in (2.74 m)
Wheelbase: 6 ft 8 in (2.03 m)
Propeller diameter: 6 ft 3 in (2.03 m)
Cabin door height: 2 ft 10 in (0.86 m)
Cabin door max width: 2 ft 9 in (0.84 m)
Baggage compartment door height: 2 ft 0 in (0.61 m)
Baggage compartment door width: 1 ft 8-1/4 in (0.51 m)


Areas
Wings, gross: 161.5 ft? (15.00 m?)
Ailerons (total): 11.77 ft? (1.09 m?)
Trailing-edge flaps (total): 16.16 ft? (1.50 m?)


Weight
Weight empty: 2,191 1b (994 kg)
Max T/O weight: 3,325 lb (1,508 kg)

Performance
Max never-exceed speed: 196 knots (226 mph; 363 km/h) IAS
Max cruising speed (75% power): 162 knots (187 mph; 301 km/h)
Cruising speed (65% power): 156 knots (180 mph; 290 km/h)
Stalling speed, wheels and flaps down: 61 knots (70 mph; 113 km/h) CAS
Vx (best angle of climb): 70 knots (81 mph)
Vy (Best rate of climb): 94 knots (108 mph)
Max demonstrated crosswind component: 17knots (20 mph)
Max rate of climb at S/L: 1,170 ft/min (356 m/min)
Service ceiling	17,000 ft: (5,180 m)
T/O to 50 ft (15 m): 1,420 ft (433 m)
Landing from 50 ft (15 m): 1,340 ft (409 m)
Range, standard fuel, 75% power: 521 nm (600 miles; 965 km)
Range, auxiliary fuel, 65% power: 755 nm (870 miles; 1,400 km)


Comments and feedback welcome
Barry

